# createCircuitCoordConversionUTM

Function to create conversion of circuit coordinates in UTM to GPS coordinates

## Contents

- Syntax
- Description
- Inputs
- Outputs
- Example

## Syntax

    createCircuitCoordConversionUTM();

## Description

Function is a user interface that allows the user to select the UTM zone the circuit coordinates are currently in. The conversion is created for getting GPS Lat/Lon for the OpenDSS bus coordinates and the new Lat/Lon OpenDSS buscoords are saved.

## Inputs

- none

## Outputs

- none - a Circuit Conversion file is saved for any future plotting

## Example

Starts the user interface. Directions are in the interface.

    createCircuitCoordConversionUTM();