# createPVscenarioFiles

Runs the WVM model and puts out the OpenDSS PV scenario files

## Contents

- Syntax
- Description
- Inputs
- Outputs
- Example

## Syntax

    index = createPVscenarioFiles(plantInfoFile,irradianceFile,A_value,circuitFile);
    index = createPVscenarioFiles();

## Description

Function to load in the inputs to the WVM (plant info and irradiance sensor info), run WVM, create the loadshape file, and the solar scenario OpenDSS file.

## Inputs

- `plantInfoFile` - optional input with the link to the MAT file with the require PV plant information structure for WVM (see WVM.m and placePVplant.m)
- `irradianceFile` - optional input with the link to the MAT file with the require irradiance sensor information structure for WVM (see pvl_WVM.m)
- `cloud_speed` - optional input with a single value of the daily cloud speed
- `circuitFile` - optional input with the link to the file with the OpenDSS circuit

## Outputs

- none - outputs both a .txt loadshape file and a .dss solar scenario OpenDSS file

## Example

Example run of createPVscenarioFiles

    createPVscenarioFiles('./ExampleCircuit/Ckt24_PV_Central_7_5.mat','./Subfunctions/WVM_subfunctions/Livermore_irr_sensor.mat',10,'.\ExampleCircuit\master_ckt24.dss');
    %