# exampleTimeseriesAnalyses

Timeseries analysis and plots monitor values from the simulation

## Contents

- Syntax
- Description
- Inputs
- Outputs
- Example

## Syntax

    exampleTimeseriesAnalyses(basecaseFile,solarScenarioFiles);
    exampleTimeseriesAnalyses();

## Description

Example function for timeseries analysis and monitor plotting for net feeder power and switching components like LTC and capacitors. Monitors must be setup in the basecaseFile circuit definition. Place monitors in the desired locations, then use the same names in the code in this function.

## Inputs

- `basecaseFile` - optional input with the link to the OpenDSS file with the circuit.
- `solarScenarioFiles` - optional input with a cell array of links to the OpenDSS files with the solar scenarios to run

## Outputs

- none - generates several figures and saves them

## Example

Runs the basecase circuit and the distributed solar case

    exampleTimeseriesAnalyses('ExampleCircuit\master_ckt24.dss',{'ExampleCircuit\Ckt24_PV_Central_7_5.dss'})
    %